


      SETX3.64(1)                (Bull-SPS9)                SETX3.64(1)



      NAME
           setx3.64 - set a window to ANSI X3.64 emulation mode

      SYNTAX
           setx3.64

      DESCRIPTION
           Setx3.64 activates ANSI X3.64 emulation mode in the Bull-
           SPS9 Monochrome Display window in which it is executed.

           ANSI X3.64 mode can also be set by typing ESC % ! 1 .

           ANSI X3.64 mode remains in effect until Tektronix 40148tm
9           mode is activated with settek(1) or by typing ESC % ! 0 .
           ANSI X3.64 mode is the default terminal emulation mode for a
           newly opened window.

      NOTES
           ANSI X3.64 is the American National Standards Institute code
           number for terminal characteristics, such as implemented by
           the DEC VT-100 terminal.

      SEE ALSO
           settek(1), windows(3X), disp(7)































      Page 1                                          (73 A2 02MT REV1)



