***************************************
* ERX318 for 68000 2.10 Release Notes *
***************************************

January 9, 1990

FILES

     README.1ST    This file
     INSTALL.BAT   Batch file for software installation
     ERX68K.EXE    Emulator executable file
     ERX68K.HLP    Help file
     ERX68K.MAC    Standard macro file
     SETUP68K.CMD  Batch file for configure/setup
     SETUP68K.HLP  Help file for configure/setup
     STMAC68K.HLP  Help file for standard macro commands
     HLLD.DOC      Document file for High level language debugger
     HLLD68K.CMD   High level language debugger file
     HLLD68K.HLP   Help file for High level language
     HLLD68K1.CMD  High level language debugger file
     HLLD68K2.CMD  High level language debugger file
     CVT68K.DOC    Document file for CVT68K.EXE
     CVT68K.EXE    Symbol converter executable file
     SIEVEX.C      Sample C source file
     SIEVEX.ABS    Sample object file.

NEW FEATURES

  1. Continuous DUMP command

     If the end-address or length is not specified, DUMP command
     displays 64 bytes of memory.

     If no parameter is specified, DUMP command countinuously
     displays memory.

       d 100
       d
       d

  2. Continuous DISASSEMBLE command

     If no parameter is specified, DISASSEMBLE command continuously
     disassembles memory.

       di 2000
       di
       di

  3. Memory manipulation commands during emulation

     Memory manipulation commands can be used while program is
     running.

       r reset
       go
       dump 2000
       ex 1000=0ff
