          LQ-800/LQ-1000 BI-DIRECTIONAL PRINT ALIGNMENT

The LQ series printer may be electronically adjusted to compensate

for the effects of back lash in the carriage mechanism.

Re-alignment will be necessary following any work on the carriage

mechanism.


The upper case will have to be removed to allow the setting of DIP

switch SW3 on the EMMA board.


The alignment settings and procedure are different on the LQ-1500.

Its alignment is programmed into the printer's ROM.  Refer to the

Technical Manual for the alignment procedure.

                   ( Press RETURN to continue )
...
