                  NOTES ON THE LQ-800/1000/1500
                      PRINTER TEST PROGRAM

                          July  1, 1986


The LQ Printer Test Program exercises most of the features of the 
LQ-800, LQ-1000, and LQ-1500 printers.  The program may be used 
with any of the paper handling methods: continuous roll, fan-
fold/tractor feed, or individual cut-sheet/single-bin feeder.

The following files should be on the distribution diskette:

              LQ_PTP38.COM
              LQ2SCRNS.TXT
              ALN_INST.TXT
              LQ_READ.ME


                           -- NOTES --


The test runs within an 80 column width.  To exercise the full 
carriage width on -1000 and -1500 printers use the built-in self 
tests.

The bi-directional print alignment section is for LQ-800 and LQ-
1000 printers only.  Use the built-in alignment routines in the 
LQ-1500.

The skip-over-perforation test will not work properly when using 
a cut-sheet feeder.

The dashed lines in the formatting test: page length set to 1 
inch should be 1 inch apart.

The dashed lines in the formatting test: page length set to 3 
lines should be a half inch apart.

The first 4 groups in the line spacing tests should be 1 inch 
tall.