                            Getting Started !!!


     STEP 1:  Determine how you will run Jepp/Link Access software, then
              follow the instructions which apply to your computer.

              A) TO RUN FROM A HARD DISK:

                 Create a new sub-directory on your hard disk named JEPP.
                 Copy the DISTRIBUTION diskette to that sub-directory.
                 The following example assumes drive c: is the destination
                 hard disk drive and the DISTRIBUTION diskette is loaded
                 in drive a:

                      md c:\JEPP
                      copy a:*.* c:\JEPP

                 Go to c:\JEPP, type LOAD, and do as instructed.

              B) TO RUN FROM TWO 360k DISKETTE DRIVES:

                 Format three diskettes.

                      Label the first:      DOCUMENT/TUTORIAL
                      Label the second:     PROGRAM
                      Label the third:      DATA

                 Load the DISTRIBUTION diskette in drive a:, type LOAD at
                 the a: prompt, and do as instructed.

              C) TO RUN FROM A SINGLE DISKETTE (720K OR GREATER ONLY):

                 Format a single diskette.

                      Label the diskette:   DOCUMENT/TUTORIAL/PROGRAM

                 Copy the DISTRIBUTION diskette to the DOCUMENT/TUTORIAL/
                 PROGRAM diskette.


     NOTE:  Run Jepp/Link Access from your newly created and labeled
            diskette(s) or hard disk. PUT THE ORIGINAL DISTRIBUTION
            DISKETTE IN A SAFE PLACE!


     STEP 2:  Review the user guides and do the tutorial.

              Load your DOCUMENT/TUTORIAL or DOCUMENT/TUTORIAL/PROGRAM
              diskette in drive a: or, if Jepp/Link Access is on a hard
              disk, make the JEPP sub-directory CURRENT.  Type START at
              the DOS prompt.  The Jepp/Link Access main menu will be
              displayed.  Menu selections include:  GETTING STARTED,
              which duplicates this installation procedure and exists
              as READ.ME on disk, JEPP/LINK ACCESS SOFTWARE USER GUIDE
              and JEPP/LINK SERVICE USER GUIDE, both of which can be
              printed, and the JEPP/LINK TUTORIAL, an interactive
              offline introduction to the Jepp/Link service.  Although
              Jepp/Link is simple and straightforward, the procedures
              and their expected outcomes will be better understood after
              viewing the tutorial.


     STEP 3:  Run Jepp/Link Access Software.

              To run Jepp/Link Access software on a hard disk, type START
              at the DOS prompt and select JEPP/LINK at the menu.

              To run Jepp/Link Access software from a single diskette,
              follow the same procedure as the hard disk user, but execute
              the following DOS command before starting Jepp/Link Access:

                      assign b=a

              To run Jepp/Link Access software from two diskette drives,
              load the PROGRAM diskette in drive a: and the formatted
              diskette labeled DATA in drive b:.  Make drive a: CURRENT.
              Type START, then select JEPP/LINK from the menu.

     NOTE: Jepp/Link Access software was written to run directly under
           DOS.  If you use a TSR-type menuing system to execute Jepp/Link
           Access, results are unpredictable.  The first time you use the
           software (initialization), it is best to run it directly
           under DOS.  Experiment only after successful installation.


    STEP 4:   Jepp/Link Access Initialization

              The first time Jepp/Link Access is executed, it will
              configure itself automatically to your hardware (initialize).
              Before starting the initialization process, CONNECT AND TURN
              ON YOUR MODEM.  TURN OFF YOUR PRINTER.  You will be asked a
              number of questions about your hardware environment.
              Initialization may be ABORTED at any time by pressing the
              Esc key.  Once the system configuration has been written to
              disk, however, the results of the configuration can only be
              modified through the SYSTEM CONFIGURATION screen at the
              UTILITY MENU in Jepp/Link Access.

              The two problems most likely to occur are the inability of
              of Jepp/Link Access to detect a Hayes-compatible modem and
              failure to have the dial-in phone numbers properly set.
              These two situations are discussed in detail under
              "OPERATIONAL DETAILS:  INCOMPLETE INSTALLATION DUE TO
              MODEM INCOMPATIBILITY" in the Jepp/Link Access
              software user guide.

              Once installation is complete, select Item 1, JEPP/LINK,
              at the Jepp/Link Access main menu.  This connects you to
              Jeppesen DataPlan's Jepp/Link service.
