
The following controllers need special consideration.  Use the switches
documented here to get full SpeedStor compatibility (ie, INSTALL /NOTYPE).
If your controller does not appear on this list, it is most likely compatible
with SpeedStor.

CONTROLLER            SWITCHES       COMMENTS
---------------------------------------------------------------------------
Adaptec 232xA         /232xA
Adaptec 232xD         /NOTYPE        In translation mode, Use ROM
                                     to low level
Adaptec 1522                         use ROM to low level format
Corel In 2000                        Not compatible
DTC ESDI (6280)       /NOTYPE        In translation mode, Use ROM
                                     to low-level
                                     In non-translation mode, use BoundedInit
                                     less two cylinders of the drive
Fastor/Lark           /NOTYPE        Use ROM on controller to low-level
                                     Use INSTALL SYS:1 to copy hidden files
Ultrastor 12F/12C     /NOTYPE        Use ROM on controller to low-level
WD1003RA2 (RLL)       /1003RA2
WD1005                /1005
WD1006                /1006
WD1007                /1007          With BIOS disabled
WD7000 FASST                         Do not low-level format drive
---------------------------------------------------------------------------

IDE drives:  SpeedStor is compatible with the IDE interface.  If, however,
you experience problems formatting or booting from your IDE drive, check
to see if CMOS is set to a drive type which closely matches, BUT DOES NOT
EXCEED the capacity of your drive.  If you find a closer match in your CMOS
table, choose the type and re-install with SpeedStor using the /NOCMOS option.

