			   TeleDisk Version 2.14

			      August 2, 1991


    This file contains the following archives:


				 RTELE214.LZH
		  ....................|....................
		  |					  |
	      RTDB214.LZH (BIOS)		      RTDD214.LZH (DIRECT)
		 |					  |
	    tdconfig.exe			       tdconfig.exe
	    teledisk.exe			       teledisk.exe

    Please note that there are two groups of products:	DIRECT - which use
    direct diskette controller hardware access, and BIOS - which use BIOS
    routines for diskette access.

    The direct-access versions can handle the widest range of diskette
    formats and densities.  However, these are limited in application by
    their requirement for IBM PC-compatible diskette hardware.	Some
    diskette adapters, most notably the Diskette Adapater/A used for
    external 5.25" drive support on the IBM PS/2 systems, are not supported
    by the direct-access versions.

    Just about any diskette hardware, however, will operate with the BIOS
    versions of these products.	 The image files produced by the BIOS and
    direct-access versions of TeleDisk are interchangeable; that is, an
    image file produced by a direct-access TeleDisk may be processed by
    a BIOS version, and vice-versa.
		       -------------------

			       Sydex
			  P.O. Box 5700
			Eugene, OR  97405
		     Voice:  (503)  683-6033
		     FAX:    (503)  683-1622
		     Data:   (503)  683-1385


 
