		WHAT'S NEW iN ANADISK 2.07

A bug has been corrected which sometimes caused problems with copying
high-density diskettes on systems with small sizes of extended memory.
In addition, copying of mixed-density diskettes has been improved.

		WHAT'S NEW IN ANADISK 2.06

The SHIFT+F3 (What File?) key now operates correctly while in Sector
Edit mode.  Various diskette access routines have been improved for
better timing on fast CPUs.

		WHAT'S NEW IN ANADISK 2.05

The COPY operation now uses Extended or Expanded memory to buffer
diskette data, eliminating swapping of diskettes.

Better density/recording mode change detection has been incorporated
in the SCAN operation.

		WHAT'S NEW IN ANADISK 2.04

More bug fixes in the file handling, especially with subdirectories.

ADINSTAL has been renamed ADCONFIG--configuration of ANADISK is now
optional.

		WHAT'S NEW IN ANADISK 2.03

We've made the files handling somewhat more robust and revised the type
analsys code so that HP 110 and Portable+, as well as Apricot diskettes
can be handled.

		WHAT'S NEW IN ANADISK 2.02

We took care of a rather obscure bug where a disk-to-disk copy is being
performed from a primary controller to a secondary.


		WHAT'S NEW IN ANADISK 2.00

In short, everything.

No kidding, AnaDisk 2.0 is a major rework of the basic product.	 Read the
documentation carefully--but if you get lost, AnaDisk has help for just
about any situation, just press F1 when you feel lost.

As usual, if you experience any problems, please let us know.

			Sydex
		153 North Murphy Ave.
		Sunnyvale, CA  94086
	       (408) 739-4866 (voice)
	       (408) 738-2860 (bbs)
