TYPE="MSD"
FUNCTION="Standard Interface"
TYPE="FPYCTL"
CHOICE="Primary Address"
SUBTYPE="CMOS=260300"
LINK
PORT=03F0h-03F5h
PORT=03F6h-03F7h
SHARE="MSD"
IRQ=6
CHOICE="Disabled"
SUBTYPE="CMOS=260301"
DISABLE=YES
FUNCTION="Drive A"
TYPE="UNIT0,FPYDRV"
HELP="Select the type of diskette drive that is installed in your
system.  If you are unsure of the diskette drive type, contact your
Authorized Compaq Computer Dealer."
CHOICE="1.44-Megabyte (3.5 inch)"
SUBTYPE="TYP=4;CMOS=10F040+140101"
CHOICE="1.2-Megabyte (5.25 inch)"
SUBTYPE="TYP=2;CMOS=10F020+140101"
CHOICE="Not Installed"
SUBTYPE="TYP=0;CMOS=10F000+140100"
FUNCTION="Drive B"
TYPE="UNIT1,FPYDRV"
HELP="Select the type of diskette drive that is attached to your
system.  If you are unsure of the diskette drive type, contact your
Authorized Compaq Computer Dealer."
CHOICE="Not Attached"
SUBTYPE="TYP=0;CMOS=100F00+14C000"
CHOICE="1.2-Megabyte (5.25 inch)"
SUBTYPE="TYP=2;CMOS=100F02+14C040"
CHOICE="1.44-Megabyte (3.5 inch)"
SUBTYPE="TYP=4;CMOS=100F04+14C040"
CHOICE="360K (5.25 inch)"
SUBTYPE="TYP=1;CMOS=100F01+14C040"
