SVGA Change Log
---------------

1.12	Added /s switch for single image view mode.
	Added multiple single image viewing from command line.
	Added AcuMOS, Avance Logic, New Cirrus, Diamond SpeedStar 24/24X,
	Genoa 7900, MXIC, Primus, RealTek, New S3.
	Added HiColor/TrueColor RAMDAC detection and support for most cards.
	Added HiColor/TrueColor VESA support.
	Added full support for 4DOS 4.0 file descriptions.
	Added 4DOS long description support.
	Added optionless path switching from command line.
	Added support for .. directories under Novell Netware.
	Added /g switch to disable character graphics.
	Added /i switch	to use initial detected video mode.
	SVGA now correctly detects initial video mode.
	Changed S_F10 in viewer to A_F10 to conform to documentation.
	VESA detection/utilization works correctly for non-64K granularities.

1.11	Added SVGATEMP variable.
	Added a check for missing EMS page frame.
	Corrected Trident 8800 memory detection.
	Redesigned EMS/XMS identity determination code.
	Corrected minor video bug in exit cleanup code.
	Corrected mode listing for Video7 1024i adapters.
	Added full support for Oak 037C/067/077, including Oak HiColor.

1.10	Added Truevision TARGA support, types 1, 2, 9, and 10.
	Added 24 bit PCX, BMP support.
	Added S3 GUI Accelerator, HiColor support.
	Added Trident TVGA 8900C, 9000, LCD9100, LX9200 detection.
	Added VESA TrueColor extensions support.
	Added automatic resolution selection.
	Added accurate detection of ATI 1MB, gate version through rev 6.
	Added Tseng 4000 HiColor support.
	Added ATI 640x480x32k, 800x600x32k HiColor support.
	Added 386 detection/support.
	Added ability to display incomplete images.
	Added command line switch to force use of VESA interface.
	Added accurate video memory detection for Tseng3000 and VESA.
	Now selects native chipset in preference to VESA.
	Maximum number of files increased to ~925.
	Virtual memory errors are both clearer and less likely.
	Fixed Paradise 800x600 unsupported mode problem.
	Fixed Oak detection.

	Note:	I have completly rewritten the video adapter detection code.
		PLEASE report if you have ANY problems with adapter detection,
		such as incorrect video memory, incorrect adapter, or
		incorrect image display.

	Note:	No image quantization or dithering is currently performed.
		It is possible that it will be implemented in the future to
		improve display quality.  I chose speed over quality for this
		first truecolor version.

	Note:	HiColor modes on my ET4000 have problems with random pixels
		written to the video buffer.  This shows up while scrolling
		as image corruption, snow, etc.  This is not a software bug.
		Your mileage may vary.

1.02	No longer locks up when insufficient XMS memory is present when
	using HIMEM.SYS.

1.01	Images are now correctly displayed under low memory conditions.
	Situations where allocated disk space did not match reported disk
	space are now handled properly.

1.00	First release
