                           TeleDisk Version 2.15

                              April 16, 1992


    This file contains the following archives:


                           RTELE215.LZH
           .....................|............................
           |                          |                     |
   RTDB215.LZH (BIOS)         RTDD215.LZH (DIRECT)    RTDCH215.LZH
          |                           |                     |
     tdconfig.exe                tdconfig.exe          tdcheck.exe
     teledisk.exe                teledisk.exe          tdcheck.doc

    Please note that there are two groups of products:  DIRECT - which uses
    direct diskette controller hardware access, and BIOS - which uses BIOS
    routines for diskette access.

    The direct-access version can handle the widest range of diskette
    formats and densities.  However, these are limited in application by
    their requirement for IBM PC-compatible diskette hardware.  Some
    diskette adapters, most notably the Diskette Adapater/A used for
    external 5.25" drive support on the IBM PS/2 systems, are not supported
    by the direct-access versions.

    Just about any diskette hardware, however, will operate with the BIOS
    versions of these products.  The image files produced by the BIOS and
    direct-access versions of TeleDisk are interchangeable; that is, an
    image file produced by a direct-access TeleDisk may be processed by
    a BIOS version, and vice-versa.
                       -------------------

                               Sydex
                          P.O. Box 5700
                        Eugene, OR  97405
                     Voice:  (503)  683-6033
                     FAX:    (503)  683-1622
                     Data:   (503)  683-1385


 
