
                QEMM Version 7.0 - READ.ME File

  Congratulations!  You have just installed the most powerful,
  feature-packed memory manager available for 386, 486, and Pentium-
  based PC's.  Please take a moment to review this text file which
  includes a few tips to help you get the most out of QEMM as well
  as some last-minute information that did not make it into the
  manual.   You may want to print this file for future reference.
  To do this type "COPY READ.ME PRN:" at the DOS prompt.

                    QEMM SETUP - Check it Out!

  If you have used earlier versions of QEMM, you may be used
  to manually editing your CONFIG.SYS file to add or remove
  QEMM parameters--and paging through the manual for help in
  determining which ones you need and why.  Those days are gone.

  QEMM has a new feature called QEMM Setup that lets you quickly 
  and easily make changes to QEMM.  QEMM Setup also contains
  valuable information about getting the best use of QEMM, using
  QEMM with different hardware, software and versions of DOS, and
  troubleshooting information.
 
  To run QEMM Setup, just type QSETUP at the DOS prompt. QEMM Setup
  does all this and more:

  1)  Enables or disables the features you choose, adding the
      appropriate lines to your CONFIG.SYS file.

  2)  Adds or removes some of the more commonly-used QEMM 
      parameters and explains what they do and when to use them.

  3)  Provides extensive online help, including detailed
      explanations of many features and parameters.

  4)  Allows you to manually edit your CONFIG.SYS or AUTOEXEC.BAT
      file, without leaving QEMM Setup.

  5)  Lets you view hints and tips, this READ.ME file, and a
      collection of troubleshooting and informational technotes.

  6)  Tells you if you need to run QEMM's Optimize program after
      changing your configuration--and then runs it for you.

  With the addition of QEMM Setup, you not only have the most 
  powerful memory manager, but the easiest one to use.


                    GENERAL INFORMATION

  STEALTH ROM and STEALTH DOUBLESPACE - Use of EMS Page Frame:

  QEMM's Stealth ROM and Stealth DoubleSpace (ST-DBL) features
  depend on the existence of an EMS page frame. QEMM installation
  normally sets up a page frame in upper memory. If you want to
  use the Stealth features, you must do nothing that would
  eliminate the page frame (i.e., do not use the parameters EMS:N;
  FRAMELENGTH=0, 1, 2 or 3; or FRAME=NONE on the QEMM386.SYS
  device driver line in CONFIG.SYS.)


                    TROUBLESHOOTING QEMM

  You will find general troubleshooting information in Appendix A
  of the QEMM manual. There are also several technical bulletins
  included in the \QEMM\TECHNOTE directory on your hard drive.
  These "technotes" cover a variety of issues such as Exception 13
  messages and using QEMM with Microsoft Windows, Stacker and
  other programs. For information on the technotes, see Appendix B
  of the QEMM manual.  You can view the technotes from the QSETUP 
  program or from within your favorite text editor or viewer.


                   COMPATIBILITY ISSUES

  QEMM is compatible with almost all popular hardware and software.
  Although compatibility problems are rare, we have compiled a list
  of hardware and software products that require parameters,
  excludes, etc. when used in conjunction with QEMM or Stealth ROM.
  If you have problems with a specific program or with your system
  after installing QEMM, you should refer to the technical bulletin
  PRODUCTS.TEC for information on resolving compatibility issues.
  This technote can be found in your QEMM\TECHNOTE directory.  You
  can view it from the QSETUP program or from within your favorite
  text editor or viewer.


           DISK COMPRESSION SOFTWARE AND OPTIMIZE

  QEMM now has automatic support for Stacker versions 2.0 - 3.1
  and SuperStor 2.0, 2.04 and SuperStor Pro.  If you use either
  of these disk compressors, see the appropriate technote file
  (STACKER3.TEC or SSTOR.TEC).  These files are located in the
  QEMM\TECHNOTE directory.  You can view them from QSETUP program
  or from within your favorite text editor or viewer.

  If you are using XtraDrive, refer to XTRADRV.TEC.

  If you are using DoubleDisk Gold, read DBLDISK.TEC.

  Space MANAger by Vertisoft is not compatible with QEMM's new
  Stealth DoubleSpace feature.  DO NOT use Stealth DoubleSpace
  (ST-DBL) if you are using this program.  Doing so can result
  in loss of data on your hard drive.


                      OPERATING SYSTEMS

  MS-DOS 6:

  MS-DOS 6 gives you the ability to create multiple CONFIG.SYS and
  AUTOEXEC.BAT blocks and choose from the various configurations
  at boot up.  QEMM 7's Optimize supports this feature of DOS 6 by
  allowing you to choose which configuration you wish to Optimize.
  For more information on running Optimize while using multiple
  configurations, see the text file MSDOS6.TEC in the QEMM\TECHNOTE
  directory.  You can view it from the QSETUP program or from
  within your favorite text editor or viewer.

  DR DOS 6:

  For information on optimally configuring DR DOS 6 with QEMM 7 and
  DOS-Up, see the file DRDOS6.TEC in the QEMM\TECHNOTE directory.
  You can view it from the QSETUP program or from within your
  favorite text editor or viewer.


                           NEW PARAMETERS

  XBDA:x (QEMM386.SYS parameter)

  By default, QEMM detects the Extended BIOS Data Area (XBDA) on
  systems that have it, and moves it away from the top of
  conventional memory to a place in High RAM. However, if QEMM
  detects that you have a Suspend/Resume feature, or if you place
  the SUSPENDRESUME parameter on the QEMM386.SYS line in CONFIG.SYS,
  it will by default move the XBDA into conventional memory.
  (This is done in order to retain the use of the Suspend/Resume
  features.)  QEMM will also place the XBDA in conventional memory
  if there is no available High RAM.  When the XBDA is in High RAM
  or conventional memory, QEMM is still able to perform video
  filling on monochrome, Hercules and CGA systems.  Moving the XBDA
  does not prevent the use of VIDRAM on EGA/VGA systems, nor does
  it reduce the size of DESQview or DESQview/X windows by 16K.

  The XBDA:H parameter forces QEMM to put the XBDA in High RAM
  (if there is any available) even if you have a Suspend/Resume
  feature.  This parameter can save you 1K of conventional memory,
  but you risk Suspend/Resume not working properly.

  The XBDA:N parameter tells QEMM not to move the XBDA.  XBDA:N is
  a common troubleshooting option, and is needed whenever a ROM or
  an application assumes that the XBDA is located at the top of
  conventional memory.  The symptom of this problem is usually a
  system crash, which can occur at boot time or later, or a failure
  to access a disk.

  The XBDA:L parameter forces QEMM to move the XBDA to low
  conventional memory instead of High RAM; this decreases
  conventional memory by 1K, but preserves all the other benefits
  of moving the XBDA.  This parameter is therefore a less drastic
  solution to XBDA-related problems than XBDA:N, although XBDA:N
  will solve some problems that XBDA:L will not.


  LOADHI.COM /ENVHI (or /EH)
  (LOADING THE DOS ENVIRONMENT INTO UPPER MEMORY)

  There is a new LOADHI.COM parameter, /ENVHI (abbreviated /EH),
  that is used to load the command processor and the DOS environment
  into upper memory.  Because many network shells will fail if the
  environment is loaded high, you should only use this parameter
  if you are NOT using a network.

  QEMM's DOS-Up feature normally loads your command processor into
  upper memory by adding LOADHI.COM to your SHELL statement in the
  CONFIG.SYS file.  With the LOADHI.COM syntax added, your SHELL
  statement would look something like this (with the n in R:n
  replaced by a High RAM region number):

  SHELL=C:\QEMM\LOADHI.COM /R:n C:\DOS\COMMAND.COM C:DOS\ /E:2048 /P

  DOS's default environment size is 160 bytes. If you need more
  conventional memory (and, especially if you are using the /E:
  switch on your SHELL line to create a larger environment) you may
  want to add the /ENVHI parameter to have QEMM load the command
  processor and the DOS environment into upper memory as follows:

  SHELL=C:\QEMM\LOADHI.COM /ENVHI /R:n C:\DOS\COMMAND.COM
         C:\DOS\ /P /E:2048

  In the above example, the /ENVHI parameter would gain you an
  extra 2K of conventional memory by loading the environment into
  upper memory.  (NOTE:  In our example above, all parameters
  should be typed on the same line.)


               FILES CREATED AND USED BY OPTIMIZE

  HINTDATA.OPT - Used by MANIFEST after the OPTIMIZE process for
  providing optimization hints.

  UNOPT.BAT - Restores CONFIG.SYS and AUTOEXEC.BAT as they existed
  before you most recently ran Optimize.  Requires the presence of
  the AUTOEXEC.QDK and CONFIG.QDK files created by OPTIMIZE.

  OPTIMIZE.INF - User-readable file that contains information
  about the OPTIMIZE process.

  OPTIMIZE.DAT - Data file that holds information used when
  processing called .BAT files.

  LOADHI.OPT - Output file generated by the LOADHI programs during
  the Detection Phase and processed by OPTIMIZE during its
  Analysis Phase.



                  CORRECTIONS TO QEMM MANUAL
  
  P. 20 In the third paragraph in the section "Booting Without 
  QEMM," the last sentence should read:
  
    If you are using QEMM's DOS-Up feature, you will see a message 
    asking if you want to unload it; press Esc to unload DOS-Up, 
    then IMMEDIATELY press and hold down Alt again.   

  P. 22 Near the bottom of the page, the line that loads QEMM's 
  DPMI driver should appear as follows (all on a single line):

   DEVICE=C:\QEMM\LOADHI.SYS /R:n C:\QEMM\QDPMI.SYS 
       SWAPFILE=DPMI.SWP SWAPSIZE=1024

  P. 24 The fifth paragraph from the bottom of the page, concerning
  DR DOS, is incorrect. Please see the text file DRDOS6.TEC in the
  QEMM\TECHNOTE directory for information on using QEMM with 
  DR DOS 6. You can view it from the QSETUP program or from within 
  your favorite text editor or viewer.

  P. 39 The second paragraph should read:

    DOS-Up will modify it to read:
    SHELL=C:\QEMM\LOADHI.COM /r:x C:\DOS\COMMAND.COM C:\DOS\ /P

  P. 56 In the description of the RAM parameter, the first sentence
  of the second paragraph should read:

    If you specify the RAM parameter without an address range, QEMM
    sets aside room for an EMS page frame (unless you are using the
    EMS:N, FRAMELENGTH=0, 1, 2, or 3, or FRAME=NONE parameters) and
    places High RAM at all other upper memory addresses at which
    QEMM has not detected ROM, video RAM and adapter RAM.

  P. 89 The LOADHI parameter @[:file] has been renamed to
  /RESPONSEFILE[:file] (/RF[:file]).  @[:file] is still
  accepted by the LOADHI programs.

  P. 120 In the first paragraph of Step 6, the parameter TM:N is
  incorrectly listed as TM:M.

                       << End of READ.ME >>
