Summary Information for PC Mouse Pop-up Menu Software, Version 3.00B

TESTING:  Insert PC Mouse disk in drive A, insert program disk in drive B, and
type:
	A>TRACK

INSTALLATION:  Insert PC Mouse disk in drive A, insert program disk in drive
B, and type:
		A>INSTALL

USAGE WITH INSTALLED DISK:  Boot the program disk with the mouse software
installed, or insert the program disk and type one of the following:

		A>MOUSE ProgramName
	  or	A>MOUSE ProgramName Filename

USAGE WITH TWO STAGE BOOT: Boot the PC Mouse disk, and type one of the
following:

		A>SETUP ProgramName

Then insert the appropriate program disk and run the desired program.

DISABLING THE POP-UP DRIVER:  Insert PC Mouse disk in drive A, and type:

		A>MOUSESYS /S

RUNNING THE MENU COMPILER:  Copy MSC.COM, MOUSESYS.COM, and SETUP.BAT to a
work disk.  Create or modify the file M_Program.MSC.  Type:

		A>MSC M_Program		to invoke the compiler
		A>SETUP Program		to load the .COM file into memory

MSMOUSE DRIVER INSTALLATION:  Insert PC Mouse disk in drive A, and type:

		A>MSMOUSE		for implicit COM port assignment
		A>MSMOUSE /1		for standard COM1: configuration
		A>MSMOUSE /2		for standard COM2: configuration
		A>MSMOUSE /D		for Davong COM2: configuration

or use the INSTALL command (easier).

MSMOUSE DEVICE (DOS 2.00):  Add the following line to the CONFIG.SYS file:

		DEVICE=MSMOUSE.SYS /x

where x is either 1, 2, or D to specify the COM port.  Put before any other
DEVICE references.  (Remember to copy the file MSMOUSE.SYS to your DOS
diskette or hard disk).


ADDITIONAL ASSISTANCE:  Insert PC Mouse disk in drive A, and type:

	A>VIEW README.TXT	for detailed installation and usage info
	A>VIEW CONTENTS.TXT	for a description of diskette contents

