 INSTALLATION:

 OPTION 1:

 TWO 1.44 FLOPPY DISK ARE REQURIED FOR THIS INSTALLATION.

 1. UNZIP ALL FILES FROM CRK793A.ZIP TO FLOPPY DISK 1.
 2. UNZIP ALL FILES FROM CRK793B.ZIP TO FLOPPY DISK 2.

 RUN INSTALL.EXE FROM DISK 1.


 OPTION 2:

 CREATE A DIRECTORY ON YOUR HARD DRIVE CALLED CRACKS (OR WHATEVER YOU CHOOSE)
 ANYTHING BUT --> CRACKS93.

 1. UNZIP ALL FILES FROM CRK793A.ZIP TO THE CRACKS DIRECTORY.
 2. UNZIP ALL FILES FROM CRK793B.ZIP TO THE CRACKS DIRECTORY.

 THE FILE --> FILE_ID.DIZ <-- IS ABOUT THE SAME AND IS MENT MORE FOR
 BBS'S, SO DONT WORRY ABOUT OVERWRITING ONE ANOTHER.

 RUN INSTALL.EXE.
