                        PADLOCK for FALCON/MIG/HORNET
                               Version 1.03
                        By: Ken "Stinger" Richardson
                              UID: [70761,301]
                         InterNet: krichar@fox.nstn.ns.ca

        PADLOCK is a terminate and stay resident program that will add small 
indicator lights to the Padlock and "Scrolled up" views. These lights 
indicate Afterburners, AirBrake, Radar, and ECM. Each indicator has it's own 
color for easy identification. 

No modification is required to the Host program. Simply run the PADLOCK
program, or use LOADHIGH to load it into high memory. After PADLOCK is loaded
it will automatically check to see if a Host is running. If a Host is running
it will automatically "attach" itself. If a Host is not running, it will 
simply lay dormant in memory until it senses a Host. To Un-install PADLOCK, 
just execute the PADLOCK.COM program a second time. This will remove the TSR 
from memory.

PADLOCK also has a feature that will allow you to remap your COM3 and COM4
ports to COM1 and COM2 respectively. This will allow people to connect
in one of the communications modes using COM3 or COM4. To enable the
COM port remap feature, add the /3 or /4 switch after typing PADLOCK. For
example: Type PADLOCK /3 to remap COM3 to COM1
           or PADLOCK /4 to remap COM4 to COM2

PADLOCK will work for all versions of Falcon 3.0 after version 3.01.1, all         
versions of MiG-29 after version 1.00, and all versions of Hornet from
Spectrum Holobyte.

        This utility is not supported by Spectrum Holobyte in any way so if
you experience any problems contact me via Compuserve EMail or the MODEMGAMES
forum on Compuserve (GO MODEMGAMES).

                                        -Enjoy!

                                         Stinger

File list:
              PADLOCK.COM - Padlock TSR itself. This file must be loaded before
                            running the simulators.
              PADLOCK.TXT - This file.
       


