Turbo Assembler  Version 4.1  Copyright (c) 1988, 1996 Borland International
Syntax:  TASM [options] source [,object] [,listing] [,xref]
/a,/s          Alphabetic or Source-code segment ordering
/c             Generate cross-reference in listing
/dSYM[=VAL]    Define symbol SYM = 0, or = value VAL
/e,/r          Emulated or Real floating-point instructions
/h,/?          Display this help screen
/iPATH         Search PATH for include files
/jCMD          Jam in an assembler directive CMD (eg. /jIDEAL)
/kh#           Hash table capacity # symbols
/l,/la         Generate listing: l=normal listing, la=expanded listing
/ml,/mx,/mu    Case sensitivity on symbols: ml=all, mx=globals, mu=none
/mv#           Set maximum valid length for symbols
/m#            Allow # multiple passes to resolve forward references
/n             Suppress symbol tables in listing
/os,/o,/op,/oi Object code: standard, standard w/overlays, Phar Lap, or IBM
/p             Check for code segment overrides in protected mode
/q             Suppress OBJ records not needed for linking
/t             Suppress messages if successful assembly
/uxxxx         Set version emulation, version xxxx
/w0,/w1,/w2    Set warning level: w0=none, w1=w2=warnings on
/w-xxx,/w+xxx  Disable (-) or enable (+) warning xxx
/x             Include false conditionals in listing
/z             Display source line with error message
/zi,/zd,/zn    Debug info: zi=full, zd=line numbers only, zn=none