
CDFILE/2-20 CD-ROM Jukebox Manager

- Supports OS/2 Warp and OS/2 LanServer

- Single Drive Letter CD's as Subdirectories

- Fully transparent access

- Multiuser network solution

- Advanced Directory Caching

- Supports (up to 20 CD's) Jukeboxes (PIONEER DRM-1804X)


- up to 1000 CD's solutions available

copy CDFILE.SYS , CDFILE.IFS , CDBDLL.DLL to C:\


Apply the following changes to config.sys

BASEDEV=OS2ASPI.DMD

SET CDFILE=D:\CDFILE
DEVICE=C:\CDFILE.SYS
IFS=C:\CDFILE.IFS /MWT:3000
RUN=D:\CDFILE\CDFILE.EXE F

For Adaptec (non PS/2) user's include the /ET option
  BASEDEV=AHA154X.ADD  /ET



In the above example F is the drive where the Jukeboxdrive
is seen by the system. Y is the mapped volume where all
the CD's are shown as Subdirectories.

To register CD's run CDREG Y F 1
   Register CD in Slot 1 using drive F with Jukeboxvolume Y

To deregister CD's run CDUREG Y 1

The cdregister utility generates a DIS???.CDF for each disk
with about 100KB - 500KB in size.

To mount the mapped volume run CDMOUNT Y
To unmount the mapped volume run CDUMOUNT Y

You may run the CDFILE.EXE manager software from within (as shown above)
yout config.sys or start it separate.


The Demo version allows for 4 CD's


  Call CD-TEK CA.,USA Fallbrook De Luz Road 1361
  Phone: 619-7231324
  Fax:   619-7284874


