# Amiga 1000 Ramex

(At the computer)

60 PIN EDGE CONNECTOR (.156") at the computer.

Pin | Name | Description
--- | --- | ---
1 | GND | Ground
2 | D15 | Data 15
3 | +5V | +5 Volts DC
4 | D12 | Data 12
5 | GND | Ground
6 | D11 | Data 11
7 | +5V | +5 Volts DC
8 | D8 | Data 8
9 | GND | Ground
10 | D7 | Data 7
11 | +5V | +5 Volts DC
12 | D4 | Data 4
13 | GND | Ground
14 | D3 | Data 3
15 | +5V | +5 Volts DC
16 | D0 | Data 0
17 | GND | Ground
18 | DRA4 |
19 | DRA5 |
20 | DRA6 |
21 | DRA7 |
22 | GND | Ground
23 | /RAS |
24 | GND | Ground
25 | GND | Ground
26 | /CASU0 |
27 | GND | Ground
28 | /CASL0 |
29 | +5V | +5 Volts DC
30 | +5V | +5 Volts DC
A | GND | Ground
B | D14 | Data 14
C | +5V | +5 Volts DC
D | D13 | Data 13
E | GND | Ground
F | D10 | Data 10
H | +5V | +5 Volts DC
J | D9 | Data 9
K | GND | Ground
L | D6 | Data 6
M | +5V | +5 Volts DC
N | D5 | Data 5
P | GND | Ground
R | D2 | Data 2
S | +5V | +5 Volts DC
T | D1 | Data 1
U | GND | Ground
V | DRA3 |
W | DRA2 |
X | DRA1 |
Y | DRA0 |
Z | GND | Ground
AA | /RRW |
BB | GND | Ground
CC | GND | Ground
DD | /CASU1 |
EE | GND | Ground
FF | /CASL1 |
HH | +5V | +5 Volts DC
JJ | +5V | +5 Volts DC