# MSX Cassette

(At the computer)
(At the cassette cable)

8 PIN DIN (DIN45326) FEMALE at the computer.
8 PIN DIN (DIN45326) MALE at the cassette cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | GND |  | Ground
2 | GND |  | Ground
3 | GND |  | Ground
4 | CMTOUT |  | Sount Output
5 | CMTIN |  | Sound Input
6 | REM+ |  | Remote control (from relay)
7 | REM- |  | Remote control (from relay)
8 | GND |  | Ground