# VGA (9)

VGA=Video Graphics Adapter or Video Graphics Array.
Videotype: Analogue.

(At the videocard)
(At the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | RED |  | Red Video
2 | GREEN |  | Green Video
3 | BLUE |  | Blue Video
4 | HSYNC |  | Horizontal Sync
5 | VSYNC |  | Vertical Sync
6 | RGND | - | Red Ground
7 | GGND | - | Green Ground
8 | BGND | - | Blue Ground
9 | SGND | - | Sync Ground