# Motherboard Power

(At the Computer)
(At the Powersupply cables)

2x MOLEX 15-48-0106 CONNECTOR at the Computer.
2x MOLEX 90331-0001 CONNECTOR at the Powersupply cables.

## P8

Pin | Name |  | Color | Description
1 | PG | . | Orange | Power Good, +5 VDC when all voltages has stabilized.
2 | +5V | . | Red | +5 VDC (or n/c)
3 | +12V | . | Yellow | +12 VDC
4 | -12V | . | Blue | -12 VDC
5 | GND | . | Black | Ground
6 | GND | . | Black | Ground

## P9

Pin | Name |  | Color | Description
1 | GND | . | Black | Ground
2 | GND | . | Black | Ground
3 | -5V | . | White or Yellow | -5 VDC
4 | +5V | . | Red | +5 VDC
5 | +5V | . | Red | +5 VDC
6 | +5V | . | Red | +5 VDC