;KBB_CFG

;To setup special options, this file must be edited with
;a strickly text (ASCII) only editor. Then copy this file
;to your KBB.CFG file (replacing it) after you backup the
;existing KBB.CFG (rename it KBB_CFG.OLD)

;lines that begin with a semi-colon (;) are comments
;to turn off a command, put a semi-colon in column one
;to activate a command, delete semi-colon in column one

;note that active lines can have a comment at the end
;start line with NO semi-colon then at then end of active line
;you can add a comment if separated with space & semi-colon

;modem comport
;port=1
;port=2
;port=3
;port=4

;highest baud rate of modem
;baud=1200
;baud=2400
;baud=4800
;baud=7200
;baud=9600
;baud=12000
;baud=14400
;baud=19200
;baud=57600

;init string to start up modem
;init=at m1 l1 q0 x4 &c1 &d2 s0=0                   ;most 2400 baud modems
;init=at m1 l1 q0 x4 &c1 &d2 s0=0 &q0 s46=0 s95=1   ;most high speed modems
;init=atm1l1q0x4&c1&d3s0=0&q0s46=0s95=1h            ;PPI high speed FAX/modems

;answer ring with this string
;ring=ata           ; modem
;ring=AT+FAA=1;A    ; PPI FAX/modem

;connect strings (report speed caller connected with)
;don't change these unless you are expert at modem programming
14400=CONNECT 14400
12000=CONNECT 12000
9600=CONNECT 9600
7200=CONNECT 7200
4800=CONNECT 4800
2400=CONNECT 2400
1200=CONNECT 1200

;timing speeds for inactivity and logoff due to inactivity
;don't change these ... future use for high speed computers
tick=3000
tock=100
kill=10

;nick is userid of KBBS owner
;nick=

;name is real name of KBBS owner
;name=

;kbbs is the name of your KBBS
;kbbs=

;site is your site id
;site=

;pass is system password - future use
;pass=

;adv is frequency to show ads (requires mesgs in ADS forum)
;adv=5 ;show ads after 5 mins when a menu is needed
;adv=0 ;never show ads

;time allowed on system by caller status
;status=mins is the format
;new=10
;user=20
;memb=30
;paid=60
;super=60
;root=60

;credits for downloading
;credits=0 ;upload/download credits not checked
;credits=1 ;uploads earn 1 credit, credits checked before download

;credits for new callers
;new_credits=10

;door access
;door=off
