^^l~
^^b1,00,30,f,1,e~
^b^jSTNOD - Set Call Stop Flag~
^^b0~
~
^^h1~
^^if:menu~
^b^jLink: ^hNetLink~
~
^b^fAccess: ^j<N>^hode Manipulations~
        ^b^hSET/CLEAR ^jE^hrror~
        ^b^jS^het Error Flag~
        ^b^h[Range of Nodes]~
^^else~
^b^jLink: ^hNET~
~
^b^fSyntax: ^jSTNOD [Range of Nodes]~
^^end~
~
Each Node is allowed TWO unsuccessful connections per night. This
prevents you from spending obscene amounts of money trying to call a Node
who is having problems. After two bad calls are made, your board will
make no further attempts at calling this Node. If you would like to SET
this flag yourself, and stop certain Nodes from being called TONIGHT, use
this command. Enter an optional range of Nodes, else all Nodes will be
set.~
