			Some remarks for use

* There is no install program. After unpacking simply start SA53S.COM

* System Analyser is a DOS program. The best results you get in real dos.
  If you make a boot floppy, 
  with the win98se/winME/winXP DOS you get the best results.

* In a DOSBOX of Windows 95/98/ME it can hang when other programs are active. 
  Close all running applications.
  
* If the program stops while it is testing,
  look at the character in the upper right corner.
  Reset the computer and start testing with SA53/character.
  A list of possible characters and the test they represent you can find in:
   1) SA53S/?
   2) SA53S.DOC
   3) Help 1

* With more than 512MB of memory in Windows 9x/ME there is a problem with the
  DOSBOX. See 'http://support.Microsoft.com' -> Q253912

* 'Memory low' on the screen: 
   The processor cache is not measured (old processors).
   Also the PCI info is not displayed properly

* 'Not Enough memory' on the screen: 
  There are to much resident programs in the first 640KB part. 
  Put 'HIMEM.SYS' and 'EMM386.EXE RAM NOEMS' and 'DOS=HIGH,UMB' in config.sys.
  Load drivers high with 'DEVICEHIGH' and
  programs in autoexec.bat with 'LOADHIGH'.

* Read also SA53S.DOC and READ.ME

* The Y2000 test is switched off. Switch it on with /@
* The Sound test is switched off with Win 3.1. Switch it on with /O

* Needed files to run the program:
  SA53S.COM
  SA53S.XXX
  SA53S.LIC
