app
G	conf
G	conf objects
G	help,?
G	quit
G	kill
 G	exec file
 G	expression,let expr
G	show copying
G	show warranty
G	show option [name]
G	show error
G	get option [name]
G	set option name|nr value
G	set error error_name on|off|unset

sim
E	run,go,r [start [stop]]
E	stop
E	step,s
E	next,n
	gui start
	gui stop

uc
G	state
	statistic [mem [startaddr [endaddr]]
 GM	file "file"
 GM	download,dl
E	pc [addr]
G	reset
D	dump mem_type [start [stop [bytes_per_line]]
D	dump bitname...
D	dch [start [stop]]
D	dc [start [stop]]
D	disassemble [start [offset [lines]]]
 GM	fill mem_type start end data
 GM	where mem_type data...
 GM	Where mem_type data...
B	break addr [hit]
B	break mem_type r|w addr [hit]
B	tbreak addr [hit]
B	tbreak mem_type r|w addr [hit]
B	clear [addr...]
B	delete [nr...]
G	get sfr addr...
G	set memory mem_type addr data...
G	set bit addr 0|1
G	set hardware,hw cath params...
G	info breakpoints
G	info registers
G	info hardware,hw cath
G	info stack
G	info memory
G	timer add,create,make id [direction [in_isr]]
G	timer delete,remove id
G	timer get [id]
G	timer run,start id
G	timer stop id
G	timer value,set id value
	memory createchip,cchip id size cellsize
	memory createaddressspace,createaddrspace,createaspace,caddressspace,caddrspace,caspace id startaddr size
	memory createaddressdecoder,createaddrdecoder,createadecoder,caddressdecoder,caddrdecoder,cadecoder addressspace begin end chip begin
G	memory info

	s51
	
D		di [start [stop]]
D		dx [start [stop]]
D		ds [start [stop]]
