DOSDEL(1)                 UZIX Utilities                DOSDEL(1)


NAME
       dosdel - erases an MS(X)-DOS file

USAGE
       dosdel drive dosfile

DESCRIPTION
       dosdel erases one MS(X)-DOS file from standard  IBM PC/MSX
       diskettes or hard disk partitions. The file name must  use
       slashes, not backslashes, as a separator.

       A drive code of A causes the program to use /dev/dosA, for
       example, a link to /dev/fd0.  Similarly, to have hard disk
       partition 1 be DOS drive C, /dev/dosC could be a  link  to
       /dev/hd1, and so on for other drive codes. A normal device
       name may also be used instead of a drive code. And,  also,
       a drive code of A: causes the  program  to  use  /dev/fd0.
       Similarly, a drive code of C: causes the  program  to  use
       /dev/fd2. Yet, you can join drive code and dosfile in  one
       argument, as A:DOSFILE.TXT or C:FUDEBA.ASC, etc.

SEE ALSO
       dosdir(1), dosread(1), doswrite(1), cr(1), ncr(1)

AUTHORS
       Program :- Michiel Huisjes
       Documentation :- Adriano Cunha <adrcunha@dcc.unicamp.br>

DOSDEL(1)                 UZIX Utilities                DOSDEL(1)
