# RUN: llvm-mc --disassemble %s -triple=s390x-linux-gnu < %s 2>&1 | FileCheck %s

# This would be "axbr %f14, %f0", but %r14 is invalid.
#
# CHECK: warning: invalid instruction encoding
# CHECK-NEXT: 0xb3 0x4a 0x00 0xe0
# CHECK-NEXT: ^
0xb3 0x4a 0x00 0xe0

# This would be "axbr %f0, %f2", but %f2 is invalid.
#
# CHECK-NEXT: warning: invalid instruction encoding
# CHECK-NEXT: 0xb3 0x4a 0x00 0x02
# CHECK-NEXT: ^
0xb3 0x4a 0x00 0x02

# This would be "dlr %r1, %r8", but %r1 is invalid.
#
# CHECK-NEXT: warning: invalid instruction encoding
# CHECK-NEXT: 0xb9 0x97 0x00 0x18
# CHECK-NEXT: ^
0xb9 0x97 0x00 0x18
