# RUN: llvm-mc --disassemble %s -triple=thumbv7-unknown-unknown 2>&1 | grep und
# rdar://10841671

0xe3 0xbf
0xdf 0xed 0x61 0x3b
0x71 0xee 0xe0 0x1b
0x72 0xee 0xa3 0x2b
0xdf 0xed 0x60 0x0b

# This is test is dealing with a undefined condition code value of 15 in the
# above sequence of junk bytes and not allowing the disassembler to abort on
# printing the final instruction in this list.
# 
#	ittte	al
#	vldr	d19, [pc, #388]
#	vsub.f64	d17, d17, d16
#	vadd.f64	d18, d18, d19
#	vldr<und>	d16, [pc, #384]
