This is KERMIT8 for the pdp8/e, 8/f, 8/m and 8/a.
It requires at least one KL8-E or KL8-JA, but two
is recommended (one for the console, and one for
connecting out from the pdp8).
It also requires at least 16K core. A hardware clock
can be nice.

To compile KERMIT8, you will need my MACREL library,
also available from the same place you got this file.
(Hopefully.)

To compile the program, compile each .MA file separately,
the link them all together.

If you have any problems, feel free to contact me at the
following address:

	bqt@minsk.docs.uu.se

	Johnny Billquist
