Next: Gravis Ultrasound Up: device configuration Previous: Terratec EWS Contents

## Windows Sound System

Sound cards using the Crystal Codec are normally Windows Sound Systems compatible. The Gravis Ultrasound Max series has this codec aswell, but located at a non-standard port. You might have to specify the soundcard type manually.

    [devpWSS]
      link=devpwss
      wss64000=off
    ; subtype=
    [devsWSS]
      link=devswss
      wss64000=off

wss64000
  as the Crystal Analog Codec can use sample rates up to 64Khz you should enable this feature to get crystal clear sound playback.
subtype
  if your sound card is not detected automatically use this options to set it:

  0 | - | Windows Sound System
  1 | - | Gravis Ultrasound with 16bit Daughter board
  2 | - | Gravis Ultrasound Max