# Make a ext2 file using RMPrepUSB in the root of the drive (i.e. File Name=bitdefender-rw Volume Name=casper-rw)
# Place this .mnu file and the ISO in either \_ISO\MainMenu\MNU or \_ISO\Linux\MNU or \_ISO\ANTIVIRUS\MNU
# This menu will work even on an NTFS USB boot drive
# IMPORTANT: you MUST run WinContig (Ctrl+F2) before booting E2B.

# ONLY WORKS WITH 2012 ISOs with a /casper folder - use .imgPTN file for 2015+ ISOs

iftitle [if exist $HOME$/bitdefender-rescue-cd.iso] BitDefender Rescue CD with persistence\n Set Desktop, Applications - Settings - Session and Startup - General - Automatically save session on logout to save AV updates.

set ISO=$HOME$/bitdefender-rescue-cd.iso
set PER=/bitdefender-rw

if exist CD echo WARNING: Cannot use partnew command! && pause && configfile (bd)/menu.lst
# comment out the next line if you don't want it to ask the question
set /p ask=Do you want manually set the VGA Mode (Y/N) ? 
if /i "%ask%"=="Y" set ask=vga=ask || set ask=
echo
if "%E2BDEV%"=="" set E2BDEV=hd0 && pause E2BDEV forced to hd0!
#enable parttype output
debug 1
# make empty table entry in 3rd position in ptn table
parttype (%E2BDEV%,2) | set check=
debug off
set check=%check:~-5,4%
if "%check%"=="0x00" partnew (%E2BDEV%,2) 0 0 0
if not "%check%"=="0x00" echo WARNING: PTN TABLE 3 IS ALREADY IN USE - PERSISTENCE MAY NOT WORK! && pause
debug 1
if not exist %PER% echo WARNING: %PER% persistence file not found! && pause
errorcheck off
if "%check%"=="0x00" partnew (%E2BDEV%,2) 0x0 %PER%
errorcheck on
#map ptn 4 to ISO
partnew (%E2BDEV%,3) 0x0 %ISO%
map %ISO% (0xff) || map --mem %ISO% (0xff)
map --hook
root (0xff)
kernel /casper/vmlinuz boot=casper persistent noprompt iso-scan/filename=%ISO% %ask% splash
initrd /casper/initrd.gz 
