# For persistence: (File Name=q4os-rw  Volume Name=persistence)
# 1. click 'Create ext2 FS' in RMPrepUSB
# 2. Set the FILENAME     to:  q4os-rw
# 3. Set the VOLUME LABEL to:  persistence      <------ VERY IMPORTANT
# 4. Set amount of space you would like allowed to persist

#The persistence 'volume' needs a persistence.conf file added
# Boot to linux, right-click - Open Terminal window here..., and then type following 5 lines in the terminal console
#    sudo mkdir /mnt/usb
#    df      (to see which is the USB device e.g. sd3 - partition 4 should always be listed - try also sudo fdisk -l)
#    sudo mount /dev/sdb3 /mnt/usb      (always use 3)
#    echo "/ union" > /mnt/usb/persistence.conf
#    sudo umount /mnt/usb

# now reboot 

iftitle [if exist $HOME$/q4os-live-2.0.2-i686pae.iso] q4os-live-2.0.2-i686pae iso PERSISTENT\n Boot using .mnu file with persistence
set ISO=$HOME$/q4os-live-2.0.2-i686pae.iso
set PF=/q4os-rw

if "%E2BDEV%"=="" set E2BDEV=hd0 && pause E2BDEV forced to hd0!
if exist CD echo WARNING: Cannot use partnew command! && pause && configfile (bd)/menu.lst
#enable parttype output
debug 1
# make empty table entry in 3rd position in ptn table
parttype (%E2BDEV%,2) | set check=
debug off
set check=%check:~-5,4%
if "%check%"=="0x00" partnew (%E2BDEV%,2) 0 0 0
if not "%check%"=="0x00" echo WARNING: PTN TABLE 3 IS ALREADY IN USE - PERSISTENCE MAY NOT WORK! && pause
debug 1
if not exist %PF% echo WARNING: %PF% persistence file not found! && pause
errorcheck off
if "%check%"=="0x00" partnew (%E2BDEV%,2) 0x0 %PF%
errorcheck on
#map ptn 4 to ISO
partnew (%E2BDEV%,3) 0x0 %ISO%
map %ISO% (0xff)
map --hook
root (0xff)
# default username usually  user
kernel /live/vmlinuz boot=live persistence components quiet splash label username=adminq


initrd /live/initrd.img


