FBGRID(1V)

NAME
fbgrid - draw a grid on a frame buffer

SYNOPSIS
fbgrid [ -h ]

DESCRIPTION
Fbgrid is used to generate a grid on a frame buffer for purposes of aligning the monitor. By default, the device /dev/ik0l is assumed. This may be changed by setting the environment variable FB_FILE to the name of another device or file name and exporting it before execution of fbgrid. If the -h option is used, a HIRES (1024x1024x24) grid is written; otherwise a LORES (512x512x24) device is assumed.

FILE
/vld/lib/libfb.a

AUTHORS
Gary S. Moss, BRL-VLD
Michael John Muuss, BRL-SECAD