WRM's self-created help file for quelo asm


M68K takes FILE.M68, and processes macros, producing FILE.A68
A68K takes FILE.A68, and produces FILE.PRN and FILE.LTX
QLINK takes an .LNK file, like TUTOR.LNK, and links it.
/* BEGIN TUTOR.LNK

         LINK ARAM
         LINK B
         LINK E
         LINK COMMANDS
         LINK VECTMSG
         LINK BF
         LINK BM
         LINK BR
         LINK BS
         LINK BT
         LINK DC
         LINK DFDI
         LINK DUMP
         LINK GETA
         LINK H
         LINK HE
         LINK HEX2DEC
         LINK LOAD
         LINK MDDI
         LINK MMDI
         LINK MS
         LINK MTSETUP
         LINK OF
         LINK PF
         LINK RAMTEST
         LINK TM
         LINK W
         LINK X
         LINK Y
         LINK CODE68K
         LINK DCODE68K
         LINK TRAP14
         LINK YROM
         ORG  $400
         SECTION 0,1,2,3,4
         ORG  $FF0000
         SECTION 5,6,7,8,9,10,11,12,13,14
         ORG  $FF3FFA
         SECTION 15
         END

END TUTOR.LNK */

QLINK would take files aram.ltx etc and produce TUTOR.HEX and TUTOR.LST
  TUTOR.HEX is the S-record file.

IMAGE takes the .HEX S-record file and creates a binary image .IMG
SPLIT takes the .HEX S-record and splits it, producing two INTEL HEX
  files, .EVN and .ODD.

This is the way that TUTORNEW was assembled, since the HEX files compare 100%


