


      COPYFLOPPY(1)              (Bull-SPS9)              COPYFLOPPY(1)



      NAME
           copyfloppy - Copy one floppy disc to another

      SYNTAX
           copyfloppy [ -c ] [ -f ]

      DESCRIPTION
           Copyfloppy reads an entire Bull-SPS9 floppy and duplicates
           the contents on another floppy.  COPYFLOPPY reads the
           contents of one floppy and pauses to allow the user to
           remove the source floppy and insert the destination floppy.
           The system prompts the user with instructions.

           -c causes files to be moved toward the begining of the
           destination floppy, consolidating unused space near the end.

           -f causes the destination floppy to be put in Bull-SPS9
           floppy format during the duplicating, to avoid use of the
           ZERO command on the destination floppy.

           To "crunch" the files on a floppy (relocate them into
           consecutive blocks near the beginning of the floppy), use
           copyfloppy -c. When the system pauses for the second floppy
           to be inserted, leave the source floppy in the drive.































      Page 1                                          (73 A2 02MT REV1)



