


      SETTEK(1)                  (Bull-SPS9)                  SETTEK(1)



      NAME
           settek - set a window to Tektronix 4014 emulation mode

      SYNTAX
           settek

      DESCRIPTION
           Settek activates Tektronix 40148tm9 emulation mode in the
           Bull-SPS9 Monochrome Display window in which it is executed.
           The window is initially cleared, Alpha mode is set, and the
           cursor is set at the home position.

           Tektronix 4014 mode can also be set by typing ESC % ! 0 .

           Tektronix 4014 mode remains in effect until X3.64 mode is
           activated with setx3.64(1) or by typing ESC % ! 1 .

      SEE ALSO
           setx3.64(1), wgraf(3X), windows(3X), disp(7)




































      Page 1                                          (73 A2 02MT REV1)



