GROUP="Passwords"
FUNCTION="Set power-on password"
CHOICE="Disabled"
CHOICE="Enabled"
FUNCTION="Set DriveLock password"
CHOICE="Disabled"
CHOICE="High Security"
CHOICE="Maximum Security"
FUNCTION="Set network server mode"
HELP="Use the arrow keys to select the power-on state of 
the network server mode and press ENTER.  The network 
server mode protects the computer when it is operating 
as an unattended network server.  Please note that you must 
have a power-on password in order to enable network server 
mode.
Network server mode allows an unattended server to resume 
running after an interruption in power to the 
computer.  With network server mode, when the system resumes, 
it will not wait for a password to be entered at the key 
icon (oķ).  Instead, it will start from fixed disk drive C. 
However, keyboard input will not be accepted until the password 
has been entered."
CHOICE="Disabled"
CHOICE="Enabled"
FUNCTION="Set quicklock password state"
HELP="Use the arrow keys to select the desired state of the quicklock 
password state and press ENTER.  If a power-on password is 
established, then enabling the quicklock password will lock the 
keyboard when the key sequence, CTRL-ALT-L, is typed in by the 
user.  The keyboard will remain inactive until the password 
is typed in.
Note:  If the password is disabled at the power-on key prompt,
the quicklock password feature will remain active until 
the next time the system is turned on."
TYPE="OTH,QBLANK"
CHOICE="Disabled"
CHOICE="Enabled"
FUNCTION="Set quickblank state"
HELP="Use the arrow keys to select the desired state of the quickblank 
feature and press ENTER.  If a power-on password is established and
quicklock is enabled, then enabling the quickblank feature will
blank the screen when the quicklock keyboard sequence, CTRL-ALT-L, 
is typed in by the user.  The keyboard will remain inactive and 
the screen will remain blanked until the password is typed in."
CHOICE="Disabled"
CHOICE="Enabled"
ENDGROUP
