
    Date: February 18'th 1998.

    This is the official list of DOS programs I released. You can download
    the latest versions from my Web-site "http://sisenis.latnet.lv/~yelena".
    They also should be somewhere in the InterNet. Try SimTel (ftp.simtel.net)
    or Demos (ftp.demos.su), where they should be. The 'Compressed' field is
    the name of the archive files, followed by an extension such as .ZIP
    (PKZip), .LZH (LHA), or any compressor.  The 'xx' or 'xxx' represent the
    package version. All these programs include documentation in english and
    russian or latvian. If you can't find something, write me by E-mail:
    "yelena@lanet.lv". You can register all my TSRs listed below for only
    US $25,-, for 50% of price.

						Ansis

   Name:	Bremze
   Compressed:	BREMZExx (last BREMZE41)
   Size:	16 KB package and 480 bytes in memory.
   Purpose:	BREMZE (Latvian for 'brake') slows down PC performance by
		controlling the speed of execution of programs.  This feature
		can be useful when running old processor-dependent programs
		on new PCs, particularly to decrease the speed of games for
		'better results', or when wishing to gain a better understan-
		ding of the sequences and functioning of programs, etc. Big
		diapason of braking coefficients (enough to fastest PCs),
		braking level control and switch on/off by hot-keys, control
		output trough PC speeker. Full command line control. Slows
		down also Windows programs. Versions for both interrupts is
		available - 08h and 70h.


   Name:	Burti
   Compressed:	BURTIxxx (last BURTI600)
   Size:	11 KB package and 1280 bytes in memory.
   Purpose:	BURTI is a universal Latvian keyboard and EGA/VGA screen driver
		for DOS. It support all variants of keyboard input and all
		text modes with 8x8, 12x8, 14x8 and 16x8 character set. Full
		command line control.


   Name:	DosClip
   Compressed:	DOSCLIxx (last DOSCLI30)
   Size:	14 KB package and 2300 bytes + clipboards size in memory.
   Purpose:	DOSCLIP is a resident program that organizes a text clipboard
		in DOS, allowing you to copy the screen contents to the clip-
		board in ALL (extended SVGA including) text video modes and to
		paste from the clipboard to the keyboard buffer in all video
		modes. DOSCLIP is compatible with the Windows clipboard; it
		permits the export and import of text data to the Windows
		clipboard, provided Windows is active (in 386 Enhanced mode).
		Keyboard and mouse controls. Full command line control. The
		special symbols (00-31 and 127) when putted to clipboard is
		changed to spaces. The spaces at ends of lines (except last
		line) is deleted.


   Name:	DosVer
   Compressed:	DOSVERxx (last DOSVER21)
   Size:	11 KB package and 352 bytes in memory.
   Purpose:	DOSVER is a small resident program for DOS which allows to set
		DOS version number directly or automatical control requested
		DOS version. So, with DOSVER you can use programs with identi-
		cal names that need different DOS versions, at the same time.
		You can load and reconfigure DOSVER "on the fly".


   Name:	StopPrg
   Compressed:	STOPPRxx (last STOPPR33)
   Size:	10 KB package and 1440 bytes in memory.
   Purpose:	STOPPRG is a resident program that allows you to stop any pro-
		gram and exit to DOS (except programs that change the interrupt
		08h handler). It's useful in infinite cycles, in programs wi-
		thout exit, in hung-up programs with not hung-up DOS.


   Name:	UpTimer
   Compressed:	UPTIMxxx (last UPTIM400)
   Size:	9 KB package and 256 bytes in memory.
   Purpose:	Programs that use the timer interrupt, such as action games,
		resident utilities - as well as my utility BREMZE - and PCs
		running in APM energy saving mode, can cause the system timer
		to lag behind the real-time clock.  UPTIMER corrects any such
		time discrepancy by updating the system timer from the real-ti-
		me clock every second, thereby ensuring that the system timer
		and the real-time clock remain in synchronism.